OP Panel

2. FUNCTION OF EACH PART 쭬

(1) Main CPU

l) Main CPU : To control whole process for knitcom controll er

2) Main CPU Sub. : To control F-drv , Y-drv , etc.

(2) OP CPU

l) OP CPU : To control total size , LCD panel , input key pad , S/W.

2) OP CPU Sub. : To control in and out , check error.

(3) F-drive : To out-put to each actuator

(4) Y-drive : To out-put to ringlet and yarn air solenoid.< /font>

(5) Power : 5V, 12V, -l8V, 28V switching mode power

(6) FDD : This function receives pattern data designed by PDS by

controlling FDD.

(7) Encoder : To recognize the current position by receivin g the change

of encoder signal according to the revolution for machine.< /font>

(8) Limit Switch : To Sensing the signal from cycle S/W

This is for sensing the current knitting position of machin e (in old type)

3. Composition of operation panel

① | Display LCD
② | Keyboard
③ | Controller On/Off S.W
④ | Motor On / Off (Inverter On/Off)
⑤ | High/Low Speed S.W
⑥ | Start S.W : run machine
⑦ | Stop S.W : stop machine
⑧ | Jog S.W : inch by inch
⑨ | Keyboard ON/OFF (enable/disable)
⑩ | Quick Return S/W

<2>

Previous ; & nbsp; Next