1. ABOUT MAIN SCREEN

2. MENU

(1) MAIN-TOOLBAR
1) PRINTING
2) DUPLICATING DATA
3) OTHER BUTTON

(2) EDIT CHAIN DATA
1) READ AND WRITE FILE
2) DELETE, INSERT
3) EDIT CHAIN

(3) EDIT FIXED SELECT DATA
1) EDIT AIR CAM ACTION
2) EDIT JACQUARD DATA NOUMBER
3) CHANGE DATA ACCORDING NEEDLE COUNT

(4) OTHER FUNCTIONS
1) EDIT JACQUARD DATA
2) EDIT AIR CAM NAME

1. ABOUT MAIN SCREEN

¡¸ Screen ¡¹

1)Main toolbar : Area for main tools like as file,printing,copy,paste,,,

2)Window for chain data : Area for editing chain dat(act,size,speed,ringle i/o,,,)

3)Winfdow for FIXED SELECT dat : Area for editing fixed selection dat(air cam i/o)

4)Window for file name which editing now : Area for showing all file name.

¡ØChain file extention is 'CHA'. :set speed, size, ringle ,yarn I/O,,,

Fixed selection file extention is 'FIX'. :set in or out air cam

Jacquard file extention is 'JAC'' :set each actuator action.

If you read anyone chain data from disk then all 3 datas are need for our system.

2. Menu

(1)Main toolbar

1)Printing : To print all chain dat or air cam name

-Click 'File'->'print'

-Select one which you want.

Select 'print chain', then all chain data will be printed.

'Print air name' makes printing air name dat only for refer.

2)Duplicating data : To duplicate chain or F-S dat from one step to another step.

*

a)Move step you want for source --- click step you want.

b)Select 'Chain or F-S dat'

c)Move step you want to destination.

d)Select 'Chain or F-S dat' --- If you selected chain then select Chain, F-S selected then select F-S.

3)Another button

*

(2)Edit Chain data

1) Read and write file

*

a) 'Read file' : To read chain data from 3.5" FDD disk

Click this button and select fiel you want.

b) 'Write file' : To write chain data to 3.5" FDD disk

Click this button and input file name if new , or click file in file window if overwrite.

2) Edit chain step data

*

a)moving step

Press move up or move down button then up 1 step or down one step.

Or input step number you want on 'STEP window'.

b)Inserting one step

Move step you want(click mouse to step you want), Click 'INSERT' button.

Then one step will be insert and this step has 'No data'.

c)Delete one step

Move step you want(click mouse to step you want), Click 'DELETE' button.

Then one step will be delete and next step has come in this step.

d)Clear one step

Move step you want(click mouse to step you want), Click 'CLEAR' button.

Then one step will be clear only, and this step has 'No data'.

e)Call sub-chain : not used

f)Set 'END POINT' : To set endding point in chain data.

You must mark 'END POINT' on the end of chain data

Move the step after last step end click 'END POINT', then set end step.

(3) Edit chain data

a)Edit basic chain dat

* This is "Input button" for input data you want on the right side

¨çSet knitting position :Click position "Input button" then one screen will be showon like below.

Move cursor and select(click) position that indicate current step position.
Right button for escape.

Or press right sided down arrow mark and select in text.

¨èSet F.S number :Clicking F.S "Input button" makes apper window as below.

Input F.S No. from 1 to 37 for cam action,
or100 for pattern knitting, or 0 for wait knitting(heel toe ,,,) and click 'OK' button.

¨éInput size :To set knitting course in this step.

-Click size "Input button" , input size you want and click 'OK'.

¨êInput speed :To set knitting speed.

-Click speed "Input button" , input speed(20-450) you want and click 'OK'.

¨ëInput stitch number :To set stitch no.

Stitch No. : must be from 1 - 8 for normal. Or when tights you can use tight stitch like these, + for one by one incresaing, - for one by one decresing

¨ìInput direction : To set direction for normal or heel or toe.

Set 'F' for all knitting positionelse heel and toe.

Set 'U' for 'HEEL UP' and 'TOE UP'. 'U' means up case.

Set 'D' for 'HEEL DOWN' and 'TOE DOWN'. 'D' means down case.

Select one 'F', 'U', 'D' or automatically selected with position.

b)Set gum roller speed

*

- Button ¨Í will be appeared and disappeared whenever button ¨Î pressed.

If button ¨Í appeared then you can set gum roller speed you want. else

gum roller running in speed with controler setting.

Button ¨Í can be use for setting speed.

c)Other buttons

*

¨çD.P :Mark for down picker on off : on(green) then D.P In, else out.

¨èSDC:Mark for sole pattern on off : on(red) then sole pattern will be all plain.

¨éOIL :Mark for oil motor run or not : on(green) then oil motor run with count

¨êD.A : not used

¨ëS.O :Mark for sock out gate open or close :on(green) then open

d) Set Ringle and yarn in or out

¨çSet ringle up and down

Double click you want to set up or down and set IN(down) or OUT(up)

and input the position.

¨èSet yarn up and down

Double click you want to set up or down and set IN(down) or OUT(up)

and input the position.

'999' means no refering position for acting, it become 'I&I'.

When no IN,OUT status then no action occured.

This means ringle or yarn will be continue with before status.

(3)Edit FIXED SELECT

1)Edit air cam data

a)Edit air cam action with makes new one

-Click "insert" button for new one

And you will see as belowing.

Select air cam no. and action(IN/OUT) and position with angle(0-358) Set OK button.

b)Edit air cam action with old one.

-Double click anyone you want and same process need like as upper case.

c)Delete air cam action

-Click the air cam in window for F-S data and press the "delete" button.

¡ØWhen a cam In and out in one step then you need select twice, one is for in and another for out.

In this case that air cam will be colored in blue.

d)F.S SET button : this is for setting current F-S dat to current F-S no.

2)Edit jacquard dat.

-Jacquard No. set the dat for acting actuator when runing this F-S.

-Press each box(2C,3C,4C,5C,1F,1C) and set number for running you want.

This no. must be from 0 to 20.

And '0' means running with pattern dat and other means running with that jacquard data.

3)Select needle count and change jac. and chain data automatically.

*

Move the cursor to the area around the window on upper.

Then cursor shape will be change like '¡è'.

Click then needle count input window will be appear.

Input the needle count you want and press "OK",

Then ask automatic change or not and selecting ok or not need.

(4)Other functions

1)Editing the jacquard data

* Click the yellow button for editing jacquar data.

a)Edit data

Click then data on and off so change and make jacquard data you want.

Move jacquard no. with button for move no.

b)Copy data

-Button for copy with same dat can help you to make easy with same pat. from 1 to 256.

-Select 1 to anyone you want then same data will be repeated.

C)Block copy

-copy block data to the area you want.

-Input the no, and set 'OK' button

2) Edit air name

* Press blue button for editing air name

a) Edit name and angle

- Click button for edit name then editing window appear.

- Input the name of air cam and input the angle and press 'OK'.