## 3. Another Info.

### (1) Color map for each machine

All manufacturers use different color for their machine. But,in WinPDS,we use only one color map, and they are saving with his original color map for each company.
* Highlighted colors are for rubber pattern.
* In JW machine and 4F machines are used 2 patterns for rubber pattern. One is only pattern and another is for only rubber and in schedule of 1st pattern "Rubber" must be marked green and in schedule of 2nd pattern "Rubber" must be marked with red color.

Controller Type
| 6 F | 5 F | 4 F
F name |  | KR-6F | KR-5F | SH | KUKJEA | JUWON | HANIL | KOREA,JUWON | KUKJEA
1F | 1 YARN | BLACK | BLACK | BLACK | BLACK | BLACK | BLACK | BLACK | BLACK
2F (2C) | 1 YARN | RED COLOR | RED COLOR | RED COLOR | GRAY COLOR | BROWN COLOR | BROWN COLOR | BROWN COLOR | PUPLE
MARGENTA
2 YARN | LIGHTRED | LIGHTRED | LIGHTRED
CYAN | LIGHTMARGENT
3 YARN | LIGHTRED | LIGHTMAGENTA | LIGHTCYAN
3F (3C) | 1 YARN | BLUE COLOR | BLUE COLOR | BLUE COLOR | MAGENTA | MAGENTA | MAGENTA | MAGENTA | CYAN
LIGHTGREEN
2 YARN | LIGHTBLUE | LIGHTBLUE | LIGHTBLUE
WHITE COLOR | LIGHTRED | LIGHTCYAN
3 YARN |  | LIGHTGREEN | LIGHTGREEN
4F (1C) | 1 YARN | BROWN COLOR | BROWN COLOR | BROWN COLOR | CYAN | GRAY COLOR | GRAY COLOR | GRAY COLOR | GRAY COLOR
2 YARN | YELLOW | BROWN COLOR | YELLOW | LIGHTCYAN
5F (4C) | 1 YARN | MAGENTA | MAGENTA | MAGENTA | BROWN COLOR | BLUE COLOR | X | X | X
LIGHTCYAN
2 YARN | DARKGRAY | DARKGRAY | DARKGRAY
GREEN COLOR
3 YARN |  | LIGHTGREEN | LIGHTGREEN | YELLOW
6F (5C) | 1 YARN | WHITE COLOR | X | X | X | X | X | X | X
2 YARN | YELLOW | X | X | X | X | X | X | X
1F+3F | X | X | WHITE COLOR | X | X | X | X | X | X
1F+4F | X | X | YELLOW | X | X | X | X | X | X
YARN COLOR | NO USE | NO USE | NO USE | COLOR OF EACH F | GRAY COLOR | GRAY COLOR | GRAY COLOR | COLOR OF EACH F
RINGLET/td> | AUTOMATIC | AUTOMATIC | AUTOMATIC | GREEN COLOR |  | NO |  | GREEN COLOR
MESH | GREEN | GREEN | GREEN | BLUE | RED | RED | RED | BLUE
RUBBER | DARKGRAY | DARKGRAY | GRAY | DARKGRAY | CYAN | CYAN | CYAN | DARKGRAY

### (2) F. POSITION OF EACH MACHINE

Ringlet 1 : Nylon , Ringlet 2 : Spandex , Ringlet 3 : double sole , Ringlet 4 : Heel
Ringlet 5 : Double welt, Ringlet 6 : Rosso , Ringlet 7 : Cotton , Ringlet 8 : Cotton

1) Korea Robot 4F(SH, TH), JW 4F, KJ 4F

2) Korea Robot 5F, 6F(SH, TH, TY)

3) Kukjea 5F

4) Juwon 5F

5) TH(MK)

###

### (3) How to read pattern saved in PDS with WAC.

1. Make a pattern in PDS.
   In this case you must use another color(no white) for background .
   In schedule, START 1, END 400, REP 400. (If no sch, then no saving)
   Save this pattern in Wac disk type to 3.5"
2. Insert the disk into the WAC. computer "A drive"(Will not work in FDD for only WAC. .)
3. Select Pattern and select "A drive"
4. Select the file name you want.

### (4) Set rubber pattern for SH 5F(C7,C9)

1. In WIN-PDS,all rubber patterns are drew in right side. So, you must draw pattern in left side,and rubber in right side(X start 257 for rubber)
   And even if no rubber pattern you want, rubber (1:1, 3:3) must be in right side in WinPDS.
2. Set the schedule. as follow. ("3. Special functions (3) Set schedule " refer)
   (1) Case for no pattern in rubber

   Start | End | Repeat | G | Info.
   1 | 1 | 8 |  | Knit lylon
   2 | 2 | 100 |  | Knit rubber(repeat count must be large number:will be cancel automatically)
   4 | 400 | 800 |  | Body pattern
   Rubber | Sole | Rosso |
   N | N | N | Another info. : set all "N"

   (2) Case for pattern in rubber

   Start | End | Repeat | G | Info.
   1 | 1 | 8 |  | Knit nylon
   2 | 29 | 100 | G | Rubber pattern(repeat must be large:cancel automatically)
   32 | 400 | 800 |  | Body pattern
   Rubber | Sole | Rosso |
   Y | N | N | Another info. : set all "N"

3. When saving, select file type is " Korea Robot Inc. type" and select "5F[old]".

* For other machines, schedule for rubber part must be set with same course(KJ, JW..)

### (5)How to set needle count

1. Click the area for setting needle count in bottom area.
2. You will show window for inputting needle count.
3. Press "Enter" and move the mouse into the working area then you can see the new needle count.

### (6) Small zoom screen

1. In Toolbar Icon click that icon then the small zoom window will appear.
2. If you want change the zoom factor in ZOOM click the up or down arrow .
3. Close the small window with click once more the icon Icon.
4. Zoom factor can from 1 to 16.

   ###

Small zoom screen

###

### (7) About the GUM line info. and actuator

For T&K 5F and 6F and drumless,GUM line must be outed before rubber pattern as follow
In this case, red line means ringlet 2, blue line means ringlet 7, and two gray lines are means ringlet 1 and ringlet 8. The gray line in rightside of the blue line means GUM line.

### (8) About the changing span in pile (before 1 line)

| If you want change the nylon to span in pile, change the yarn before and set the pile as left.

### (9) About the tennis socks

| When you want tennis socks, you muse be care to set schedule. Rubber part and leg part must be divided for SH, TH, TY drum type machine (refer to following img.)

### (10) How to use HALF COPY

This function is for easy drawing with half pattern.

1. Need needle count. Usually, patterns are same with left and right side. So you can make a pattern easily with this function. Input Y course you want and X width automatically setted with needle count.
2. The rubber pattern will not copy.

   For usage, click "Half Copy"