## 2. Special functions

### (1) Making rubber pattern

Icon :

Function : To draw rubber 1:1, 3:1,, and color yarn pattern together.

Directions:

1. Click the rubber icon, and small windows will appear.

   Rubber window | Screen for RUBBER button

2. Select one you want on the screen.
3. Move the mouse and select 2 point for start point and end point like box.

   If RUBBER button, right most and bottom most area. was pressed and it's color is green then rubber pattern will be on the right side with darkgray color.

¡¼Rubber pattern making¡½

If you want rubber and color yarn knitting together, you must draw color yarn pattern on the main area(left side) and rubber pattern(Darkgray color) must be draw on the sub area(right side).And in schedule, you must make GUM is Y.(GREEN)

### (2) Making mesh pattern

Icon :

Function : To draw 1:1 or 2:1 mesh pattern.

Directions:

1. Click the mesh icon and small window will appear to select 1:1 or 2:1.
2. Select one you want.

   Mesh window | Screen for RUBBER button

3. Move the mouse and select two point for start and end point like box.

If the RUBBER button on the rib window was green then mesh pattern will be appear on the right side of the screen with darkgray color for rubber.
If the RUBBER button on the rib window was red then mesh pattern will be appear on the left side of the screen(main area) with current color..

Like this you can draw the rubber pattern , for no rubber pattern case draw only rubber 1:1 or 3:1 in left-side with "red RUBBER"

#### ¡ÚExample of rubber pattern¡Ú

.How to make a rubber pattern.
A) Draw pattern in main area with 2C,3C,4C,5C color.
B) Draw rubber pattern in sub area with rubber color(dark-gray).
rubber area starts X is 257.

C) Mark rubber to 'Y'(green) and mark 'G' on the gum side.

###

(3)Making schedule

Icon :

Function : To making schedule for pattern. This means how to knit pattern with draw.

Directions :

1. Click schedule icon.
2. You will show as belows.
   Start means Y position which you want to knit start on the screen.
   End means Y position which you want to knit end on the screen.
   repeat means total count for knitting in this times.

   | How to set the schedule
   Move the mouse to under the 'Start' line which you want and click left but. Then white cross bar will be appear on the main area. This cross bar move according to the mouse. Set cross bar to the position for starting and click left button. Now you will show Y position which you setted. Move the cursor to under the 'End' line you want and click left but. You can set the 'end position' with same method for setting 'start position. Now last step is set 'repeat'. As mentioned before, repeat means total count for knitting with pattern you want. So, if you want knitting only once from start to end position, input count in repeat area like this. Repeat count=End-Start+1: for knitting only once from start to end. Like as before, you can make all 20 schedules.(used scroll bar)

   * For other machines, you must set the rubber schedule same course.

###

(4)File format for reading and writing

Win-PDS can support SH,TH,TY,KJ,JW. So, you must select correct file type when reading or saving.

1. Window version type : not used.
2. Hard disk type(*.DAT) : Dos ver."HARD" for 4F(SH,TH)
3. Korea Robot Inc.(*.DAT) : for SH 5F,TH5,6F,TY5F
4. MK 5F type (*.YTB) : for MK 5F pattern data
5. MK 6F type(*.YTB) : for MK 6F pattern dat
6. Soosan CUT type(*.CUT) : for Soosan cut file
7. Soosan PIC type(*.PIC) : for Soosan pic file
8. Korea Robot 4F type(*.DAT) : for 4F machine(5.25" disk)
9. JW 4F type(*.DAT) : for JW 4F machine
10. JW 5F type(*.DAT) : for JW 5F machine
11. Links type(*.DAT) : for Links machine
12. Wac disk type(*.p) : for Wac controller
13. BMP data type(*.BMP) :for BMP file
14. PCX type(*.PCX) : for PCX file(640x480,16 color file only)
15. KJ ICON: Kukjea(505),(501,401), special icon

###

(5) Reading pattern from disk

Icon :

Function : To read pattern from disk.

Directions :

¨ç Select "Open"
¨è Choose the file type you want((4)File format for reading and writing), Select A,B,C.
¨é " Double click the left button or select open "

###

(6)Writing pattern to disk

ICON:

Function: How th saving the pattern to disk

Directions:

1. "Select SAVE"
2. If you want KJ then click the , else select the file type you want((4)File format for reading and writing),Select A,B,C.
3. Double click "the left-button,or select open"

<#Saving method>

1. For SH,TH,TY,SS(Korea Robot controller) 5F,6F machine.
   - Insert the 3.5" disk
   - Select save, choose the file type and position
   - Input the file name or select the old name
   - Pattern name : A~Z, 0~9,¡°_(underline)¡±max 8 char. can.

2. For Kukjea
   - Insert the KJ disk to theA(401,501) or B(505).
   - Select
   - KJ save and select from 1 to 9.

3. For JW machine
   - Insert the3.5" disk to B drive.
   - Select save, choose file type(JW 5F) and select position B.
   - Select the sub directory(0,1,2,3,,9)
   - Select the file name or input the file name.
   - File name : 0,1,2,3,4,5,6,7,8,9 can.

4. TH(for MK controller) 5F
   - Insert the 3.5" disk to B drive.
   - Select SAVE function, choose the file type(MK 5F,6F), choose B.
   - Select the file you want or input the new file name
   - file name : 0,1,2,3,4,5,6,7,8,9

###

(7) Half copy

ICON :

Function : HALF COPY

Directions :

1. "Half copy" chose will show the half copy window.
2. Y means course for copying.
3. Default is 1 - 800. Input the course you want.
4. Mirror and normal copy can.